
(module MODULE_ESP32-C3-WROOM-02-H4 (layer F.Cu) (tedit 6269D75A)
  (descr "")
  (fp_text reference REF** (at -6.575 -11.085 0) (layer F.SilkS)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (fp_text value MODULE_ESP32-C3-WROOM-02-H4 (at 7.395 11.085 0) (layer F.Fab)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (pad 1 smd rect (at -8.75 -2.9) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd rect (at -8.75 -1.4) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at -8.75 0.1) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at -8.75 1.6) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at -8.75 3.1) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at -8.75 4.6) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd rect (at -8.75 6.1) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 8 smd rect (at -8.75 7.6) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 9 smd rect (at -8.75 9.1) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 10 smd rect (at 8.75 9.1) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 11 smd rect (at 8.75 7.6) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 12 smd rect (at 8.75 6.1) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 13 smd rect (at 8.75 4.6) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 14 smd rect (at 8.75 3.1) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 15 smd rect (at 8.75 1.6) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 16 smd rect (at 8.75 0.1) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 17 smd rect (at 8.75 -1.4) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 18 smd rect (at 8.75 -2.9) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 23 smd rect (at 0.96 3.3) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 24 smd rect (at 2.06 3.3) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 22 smd rect (at -0.14 3.3) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 19 smd rect (at -0.14 2.2) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 20 smd rect (at 0.96 2.2) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 21 smd rect (at 2.06 2.2) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 27 smd rect (at 2.06 4.4) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 26 smd rect (at 0.96 4.4) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 25 smd rect (at -0.14 4.4) (size 0.7 0.7) (layers F.Cu F.Mask F.Paste))
  (pad 29 thru_hole circle (at 1.51 2.2) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 32 thru_hole circle (at 2.06 2.75) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 37 thru_hole circle (at 2.06 3.85) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 28 thru_hole circle (at 0.41 2.2) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 34 thru_hole circle (at 1.51 3.3) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 31 thru_hole circle (at 0.96 2.75) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 30 thru_hole circle (at -0.14 2.75) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 33 thru_hole circle (at 0.41 3.3) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 39 thru_hole circle (at 1.51 4.4) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 38 thru_hole circle (at 0.41 4.4) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 36 thru_hole circle (at 0.96 3.85) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (pad 35 thru_hole circle (at -0.14 3.85) (size 0.4 0.4) (drill 0.3) (layers *.Cu))
  (fp_line (start -9.0 -10.0) (end -9.0 -4.0) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 -4.0) (end -9.0 10.0) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 10.0) (end 9.0 10.0) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 10.0) (end 9.0 -4.0) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 -4.0) (end 9.0 -10.0) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 -10.0) (end -9.0 -10.0) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 -4.0) (end -9.0 -4.0) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 10.0) (end -9.0 9.87) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 10.0) (end 9.0 9.87) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 -10.0) (end -9.0 -3.67) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 10.0) (end 9.0 10.0) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 -3.67) (end 9.0 -10.0) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 -10.0) (end -9.0 -10.0) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.75 -10.25) (end -9.75 10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.75 10.25) (end 9.75 10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.75 10.25) (end 9.75 -10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.75 -10.25) (end -9.75 -10.25) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -10.5 -2.9) (end -10.4 -2.9) (layer F.SilkS) (width 0.2))
  (fp_circle (center -10.5 -2.9) (end -10.4 -2.9) (layer F.Fab) (width 0.2))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -10.0)
        (xy 9.0 -10.0)
        (xy 9.0 -4.0)
        (xy -9.0 -4.0)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -10.0)
        (xy 9.0 -10.0)
        (xy 9.0 -4.0)
        (xy -9.0 -4.0)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -10.0)
        (xy 9.0 -10.0)
        (xy 9.0 -4.0)
        (xy -9.0 -4.0)
      )
    )
  )
)