(footprint "L_Abracon_ASPI-2515" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5990349C)
  (descr "smd shielded power inductor http://www.abracon.com/Magnetics/power/ASPI-3012S.pdf")
  (tags "inductor abracon smd shielded")
  (attr smd)
  (fp_text reference "REF**" (at 0 2.6) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dc80e564-e8e5-41d3-b6a1-8ff3e4a1af0b)
  )
  (fp_text value "L_Abracon_ASPI-2515" (at 0 -2.7) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp eefaf7e0-968a-489d-b7d9-d3643badefbb)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.7 0.7) (thickness 0.105)))
    (tstamp b036c013-a245-4a30-a991-b2fcec7e2cde)
  )
  (fp_line (start -0.8 -1.6) (end 0.8 -1.6) (layer "F.SilkS") (width 0.12) (tstamp 57f8baf4-9b87-48aa-866a-d9c0607d55ab))
  (fp_line (start -0.8 1.6) (end 0.8 1.6) (layer "F.SilkS") (width 0.12) (tstamp 7c1d00b3-88ad-44d2-93db-afe0889d96af))
  (fp_line (start -2 -1.8) (end -2 1.8) (layer "F.CrtYd") (width 0.05) (tstamp 8616dc22-a59b-4382-b9b6-c5f15266836c))
  (fp_line (start 2 1.8) (end 2 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 9d97c673-0e83-45f3-ac3a-b6d60e22db19))
  (fp_line (start -2 1.8) (end 2 1.8) (layer "F.CrtYd") (width 0.05) (tstamp c37b5bf1-fe34-48c0-a857-1a2934b5e184))
  (fp_line (start 2 -1.8) (end -2 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp ea2b06df-0d2e-4e19-91df-b26251fdb678))
  (fp_line (start -1 -1.3) (end -1.5 -1.3) (layer "F.Fab") (width 0.1) (tstamp 01ab07d2-e64f-4249-a7a4-418180ea541a))
  (fp_line (start -1.5 1.3) (end -1 1.3) (layer "F.Fab") (width 0.1) (tstamp 06b3875c-eed1-4028-a2f2-454b0a854559))
  (fp_line (start 1.5 -1.3) (end 1 -1.3) (layer "F.Fab") (width 0.1) (tstamp 25c8b934-46e0-4f6e-b29d-2a71b909df9d))
  (fp_line (start -1.5 -1.3) (end -1.5 1.3) (layer "F.Fab") (width 0.1) (tstamp 32f1b1bc-df31-48e8-8399-b132d5bef110))
  (fp_line (start 0.8 -1.5) (end -0.8 -1.5) (layer "F.Fab") (width 0.1) (tstamp 399708cb-90dd-4c73-9e54-3d69c6d2ed88))
  (fp_line (start 1.5 1.3) (end 1.5 -1.3) (layer "F.Fab") (width 0.1) (tstamp 6440eaf8-17f7-4418-83a8-0d7257d3d89c))
  (fp_line (start 1 1.3) (end 1.5 1.3) (layer "F.Fab") (width 0.1) (tstamp 6aa5afb5-b8bc-4fdf-89c5-69db5a0d248c))
  (fp_line (start -1 1.3) (end -0.8 1.5) (layer "F.Fab") (width 0.1) (tstamp 7ba27bb0-a1d0-436d-b0a0-75b0624d8514))
  (fp_line (start 1 -1.3) (end 0.8 -1.5) (layer "F.Fab") (width 0.1) (tstamp afa2aee0-e635-4bc2-ad29-84f81d1bec36))
  (fp_line (start 0.8 1.5) (end 1 1.3) (layer "F.Fab") (width 0.1) (tstamp ca3f26a0-f2c7-4d6e-8145-4b2da15c57f7))
  (fp_line (start -0.8 -1.5) (end -1 -1.3) (layer "F.Fab") (width 0.1) (tstamp e9efb27d-c7c2-443f-87df-76b1ea1b1109))
  (fp_line (start -0.8 1.5) (end 0.8 1.5) (layer "F.Fab") (width 0.1) (tstamp efdfdb1e-c319-4e33-b0f0-1833a6f924d4))
  (pad "1" smd rect (at -0.85 0) (size 0.8 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 5e832197-b3f5-4d60-8a93-5c36dc953e87))
  (pad "2" smd rect (at 0.85 0) (size 0.8 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6293a389-d04c-466c-b4a8-4ce36c97f736))
  (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Abracon_ASPI-3012S.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
