(footprint "PinSocket_1x06_P2.54mm_Vertical" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A19A430)
  (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x06 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.77) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d94fd095-7a6e-4e48-86fc-cdfac8e8598a)
  )
  (fp_text value "PinSocket_1x06_P2.54mm_Vertical" (at 0 15.47) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1e2bba13-d127-4ce7-8b02-2883c591f992)
  )
  (fp_text user "${REFERENCE}" (at 0 6.35 90) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6c1c300e-2a47-4ea2-8d52-97571814b130)
  )
  (fp_line (start -1.33 14.03) (end 1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 17c8b133-a3b3-44c3-87cc-ebea86c8e707))
  (fp_line (start -1.33 1.27) (end -1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 871a4fbe-f940-4500-a093-cdab95216bb7))
  (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 95fa8ad7-bbd1-4f17-ade4-cf28dacc3dc5))
  (fp_line (start 1.33 1.27) (end 1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp ca48bb05-db96-4d1b-871e-06db7606cf80))
  (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp d5e503be-c680-43e1-84d5-dc9150a8468d))
  (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp ee57e847-5360-421c-b39c-58f88bc42d90))
  (fp_line (start 1.75 14.45) (end -1.8 14.45) (layer "F.CrtYd") (width 0.05) (tstamp b9cd561a-8485-4858-8aac-067c96aef8dd))
  (fp_line (start 1.75 -1.8) (end 1.75 14.45) (layer "F.CrtYd") (width 0.05) (tstamp c2668cb0-40a5-4fe5-8197-f2d05ce928a6))
  (fp_line (start -1.8 14.45) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c2669f11-363b-4898-a51e-b87cb2176be1))
  (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c3e11423-e935-4ab5-9cbb-0f54f009044e))
  (fp_line (start 1.27 -0.635) (end 1.27 13.97) (layer "F.Fab") (width 0.1) (tstamp 3185ad25-198a-43eb-ad35-561533eb359a))
  (fp_line (start -1.27 13.97) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 7c7b98af-8f9a-419c-a091-5fa7bd6e0be4))
  (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 82a8df90-914c-45a8-a6ed-c3d82dec4c48))
  (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 8d2306df-a16e-4b85-a70a-63e9ca761920))
  (fp_line (start 1.27 13.97) (end -1.27 13.97) (layer "F.Fab") (width 0.1) (tstamp d35a48f2-bf39-477c-8a00-05b8354abbbc))
  (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 2a8e52ae-6ffa-4b14-871d-c743e160bdeb))
  (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp a78d5ed1-9fc8-47c8-8861-16da26adfe15))
  (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 5d781fb6-49d3-4061-bf95-7a23a7ac5ec1))
  (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 94dbc264-1b26-403f-bbbe-3770ea99faa2))
  (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp fa40f122-13da-414a-a560-db828fb1be8b))
  (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp f0bf4302-52ce-45fd-8ac5-ce0a5b7f8539))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
