(module CUI_PD-30 (layer F.Cu) (tedit 5A1AB217)
  (descr "3 pin connector, PD-30, http://www.cui.com/product/resource/pd-30.pdf")
  (tags "connector 3-pin PD-30 power DIN")
  (fp_text reference REF** (at 2.5 -3.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CUI_PD-30 (at 2.5 16.15) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 2.5 6.15) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9.95 10.65) (end 9 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start 9 10.65) (end 9 14.65) (layer F.Fab) (width 0.1))
  (fp_line (start 9 14.65) (end -4 14.65) (layer F.Fab) (width 0.1))
  (fp_line (start -4 14.65) (end -4 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start -4 10.65) (end -4.95 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start -4.95 10.65) (end -4.95 0) (layer F.Fab) (width 0.1))
  (fp_line (start -4.95 0) (end -1.5 -2.35) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -2.35) (end 6.5 -2.35) (layer F.Fab) (width 0.1))
  (fp_line (start 6.5 -2.35) (end 9.95 0) (layer F.Fab) (width 0.1))
  (fp_line (start 9.95 0) (end 9.95 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start -5.29 -0.35) (end -5.29 -2.69) (layer F.Fab) (width 0.1))
  (fp_line (start -5.29 -2.69) (end -2.95 -2.69) (layer F.Fab) (width 0.1))
  (fp_line (start 10.45 -2.85) (end 10.45 15.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.45 15.15) (end -5.45 15.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.45 15.15) (end -5.45 -2.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.45 -2.85) (end 10.45 -2.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.05 10.75) (end 9.1 10.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.1 10.75) (end 9.1 14.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.1 14.75) (end -4.1 14.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.1 14.75) (end -4.1 10.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.1 10.75) (end -5.05 10.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.05 10.75) (end -5.05 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.05 0) (end -1.5 -2.45) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 -2.45) (end 6.5 -2.45) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.5 -2.45) (end 10.05 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.05 0) (end 10.05 10.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.29 -0.35) (end -5.29 -2.69) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.29 -2.69) (end -2.95 -2.69) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole rect (at 0 0 180) (size 3.7 3.7) (drill 2.7) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 5 0 180) (size 3.7 3.7) (drill 2.7) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 8.5 3.15 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 2.5 9.15 180) (size 3.2 3.2) (drill 2.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 7.15 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5 7.15 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector.3dshapes/CUI_PD-30.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
