(module JWT_A3963_1x02_P3.96mm_Vertical (layer F.Cu) (tedit 5A2A57CE)
  (descr "JWT A3963, 3.96mm pitch Pin head connector (http://www.jwt.com.tw/pro_pdf/A3963.pdf)")
  (tags "connector JWT A3963 pinhead")
  (fp_text reference REF** (at 1.91 -5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value JWT_A3963_1x02_P3.96mm_Vertical (at 1.91 6.35) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 2.2 3.7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4.6 -3.2) (end 4.6 -1.8) (layer F.Fab) (width 0.1))
  (fp_line (start -0.8 -3.2) (end 4.6 -3.2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.8 -1.8) (end -0.8 -3.2) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -0.3) (end 1.25 -1.8) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 -1.8) (end 0 -0.3) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 -2.2) (end -2.5 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.2 -2.2) (end -2.5 -2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.05 4.7) (end -2.05 -1.8) (layer F.Fab) (width 0.1))
  (fp_line (start 5.85 4.7) (end -2.05 4.7) (layer F.Fab) (width 0.1))
  (fp_line (start 5.85 -1.8) (end 5.85 4.7) (layer F.Fab) (width 0.1))
  (fp_line (start -2.05 -1.8) (end 5.85 -1.8) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 -3.55) (end 6.35 -3.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.35 -3.55) (end 6.35 5.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.35 5.05) (end -2.5 5.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.5 5.05) (end -2.5 -3.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.29 4.83) (end 5.97 4.83) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.52 4.83) (end -2.16 4.83) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.52 4.83) (end 1.52 4.57) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.52 4.57) (end 2.29 4.57) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.29 4.57) (end 2.29 4.83) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.89 -2.16) (end 4.7 -2.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.89 -3.05) (end 4.7 -3.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.97 -1.91) (end 5.97 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.16 -1.91) (end -2.16 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.89 -3.3) (end 4.7 -3.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.7 -1.91) (end 4.7 -3.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.89 -1.91) (end -0.89 -3.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.16 -1.91) (end 5.97 -1.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.16 0) (end -2.16 4.83) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.97 4.83) (end 5.97 0) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.75) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 3.88 0) (size 3 3) (drill 1.75) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector.3dshapes/JWT_A3963_1x02_P3.96mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
