(module SpringContact_Harwin_S1941-46R (layer F.Cu) (tedit 5ED60B37)
  (descr "7.25mm SMT Multi-directional Spring Contact (T+R), https://cdn.harwin.com/pdfs/S1941R.pdf")
  (tags "spring contact emi emc shield")
  (attr smd)
  (fp_text reference REF** (at -1 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SpringContact_Harwin_S1941-46R (at -1 4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -6.89 1.75) (end -6.89 -1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -6.89 -1.75) (end -3.9 -1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -5.89 1.75) (end -5.89 -1.75) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.89 -1.75) (end -6.49 -1.75) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.49 -1.75) (end -6.49 1.75) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.49 1.75) (end -5.89 1.75) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.99 -1.75) (end -6.49 -1.25) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.49 -0.75) (end -5.89 -1.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.89 -0.85) (end -6.49 -0.25) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.49 0.25) (end -5.89 -0.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.89 0.15) (end -6.49 0.75) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.49 1.25) (end -5.89 0.65) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.89 1.15) (end -6.49 1.75) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.89 1.65) (end -5.99 1.75) (layer Dwgs.User) (width 0.1))
  (fp_line (start -1.6 -2.85) (end -3.4 -2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -3.4 -2.25) (end -3.4 -2.85) (layer F.Fab) (width 0.1))
  (fp_line (start 1.2 -2.25) (end 1.2 -2.85) (layer F.Fab) (width 0.1))
  (fp_line (start 1.7 -1.75) (end 2.7 -1.75) (layer F.Fab) (width 0.1))
  (fp_line (start 1.7 1.75) (end 2.7 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -6.89 1.75) (end -3.9 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start 1.2 2.25) (end 1.2 2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -3.4 2.25) (end -3.4 2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -1.6 2.85) (end -3.4 2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -0.6 -2.85) (end 1.2 -2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -0.6 2.85) (end 1.2 2.85) (layer F.Fab) (width 0.1))
  (fp_line (start 3.2 -3.35) (end 3.2 3.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.2 3.35) (end -7.39 3.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.39 3.35) (end -7.39 -3.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.39 -3.35) (end 3.2 -3.35) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start 1.7 -2.25) (end 1.7 -1.75) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start -3.9 -2.25) (end -3.4 -2.25) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start -3.9 2.25) (end -3.9 1.75) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start 1.7 2.25) (end 1.2 2.25) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start -1.1 -2.85) (end -0.6 -2.85) (angle 180) (layer F.Fab) (width 0.1))
  (fp_arc (start -1.1 2.85) (end -1.6 2.85) (angle 180) (layer F.Fab) (width 0.1))
  (pad 1 smd rect (at -1.1 0) (size 4.6 5.7) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector.3dshapes/SpringContact_Harwin_S1941-46R.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
