(module CUI_PD-30S (layer F.Cu) (tedit 5F713184)
  (descr "3-pin nonstandard DIN connector, shielded, PD-30S, http://www.cui.com/product/resource/pd-30s.pdf")
  (tags "connector 3-pin PD-30S power DIN shielded")
  (fp_text reference REF** (at 2.5 -4.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CUI_PD-30S (at 2.5 15.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 10.55 10.65) (end 9 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start 9 10.65) (end 9 14.65) (layer F.Fab) (width 0.1))
  (fp_line (start 9 14.65) (end -4 14.65) (layer F.Fab) (width 0.1))
  (fp_line (start -4 14.65) (end -4 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start -4 10.65) (end -5.55 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start -5.55 10.65) (end -5.55 -2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -5.55 -2.85) (end -1 -2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -1 -2.85) (end 0 -1.85) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -1.85) (end 1 -2.85) (layer F.Fab) (width 0.1))
  (fp_line (start 1 -2.85) (end 10.55 -2.85) (layer F.Fab) (width 0.1))
  (fp_line (start 10.55 -2.85) (end 10.55 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start -4 10.65) (end 9 10.65) (layer F.Fab) (width 0.1))
  (fp_line (start 11.65 -3.6) (end 11.65 15.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.65 15.15) (end -6.65 15.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.65 15.15) (end -6.65 -3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.65 -3.6) (end 11.65 -3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.65 10.75) (end 9.1 10.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.1 10.75) (end 9.1 14.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.1 14.75) (end -4.1 14.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.1 14.75) (end -4.1 10.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.1 10.75) (end -5.65 10.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.65 10.75) (end -5.65 9.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.65 5.1) (end -5.65 0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.25 -2.95) (end 9.25 -2.95) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.65 0.7) (end 10.65 5.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.65 9.2) (end 10.65 10.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -3.19) (end -0.5 -3.69) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.5 -3.69) (end 0.5 -3.69) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.5 -3.69) (end 0 -3.19) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole rect (at 0 0) (size 1.6 3.5) (drill oval 0.7 2.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 5 0) (size 1.6 3.5) (drill oval 0.7 2.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 8.5 3.15) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 2.5 9.15) (size 3.2 1.6) (drill oval 2.2 0.7) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 7.15) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5 7.15) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (pad SH thru_hole rect (at -5.35 7.15) (size 1.6 3.5) (drill oval 0.7 2.9) (layers *.Cu *.Mask))
  (pad SH thru_hole rect (at -5.35 -1.35) (size 1.6 3.5) (drill oval 0.7 2.9) (layers *.Cu *.Mask))
  (pad SH thru_hole rect (at 10.35 7.15) (size 1.6 3.5) (drill oval 0.7 2.9) (layers *.Cu *.Mask))
  (pad SH thru_hole rect (at 10.35 -1.35) (size 1.6 3.5) (drill oval 0.7 2.9) (layers *.Cu *.Mask))
  (fp_text user %R (at 2.5 5.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Connector.3dshapes/CUI_PD-30S.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)