(module FanPinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19DE55)
  (descr "4-pin CPU fan Through hole pin header, e.g. for Wieson part number 2366C888-007 Molex 47053-1000, Foxconn HF27040-M1, Tyco 1470947-1 or equivalent, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
  (tags "pin header 4-pin CPU fan")
  (fp_text reference REF** (at 4 -3.55) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FanPinHeader_1x04_P2.54mm_Vertical (at 4.05 4.35) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 1.85 -1.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.35 -2.6) (end 4.4 -2.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.75 -2.55) (end 8.95 -2.55) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.95 -2.55) (end 8.95 3.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.95 3.4) (end -1.35 3.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.35 3.4) (end -1.35 -2.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.1 3.3) (end 5.1 2.3) (layer F.Fab) (width 0.1))
  (fp_line (start 5.1 2.3) (end 0 2.3) (layer F.Fab) (width 0.1))
  (fp_line (start 0 2.3) (end 0 3.3) (layer F.Fab) (width 0.1))
  (fp_line (start 5.75 -2.5) (end 8.85 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 8.85 -2.5) (end 8.85 3.3) (layer F.Fab) (width 0.1))
  (fp_line (start 8.85 3.3) (end -1.2 3.3) (layer F.Fab) (width 0.1))
  (fp_line (start -1.2 3.3) (end -1.25 3.3) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 3.3) (end -1.25 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 -2.5) (end 4.4 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0 3.3) (end 0 2.29) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 2.29) (end 5.08 2.29) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.08 2.29) (end 5.08 3.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.75 3.8) (end -1.75 -3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 3.8) (end 9.35 3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.35 -3.2) (end -1.75 -3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.35 -3.2) (end 9.35 3.8) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 2.54 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 5.08 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 7.62 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5.08 -2.16 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x04_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
