
(module XCVR_ESP32-S3-WROOM-1-N16R2 (layer F.Cu) (tedit 6279A5C0)
  (descr "")
  (fp_text reference REF** (at -6.575 -14.135 0) (layer F.SilkS)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (fp_text value XCVR_ESP32-S3-WROOM-1-N16R2 (at 7.395 14.365 0) (layer F.Fab)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (pad 41_1 smd rect (at -1.5 2.46) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 1 smd rect (at -8.75 -5.26) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_2 smd rect (at -2.9 2.46) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_3 smd rect (at -0.1 2.46) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_4 smd rect (at -2.9 3.86) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_5 smd rect (at -1.5 3.86) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_6 smd rect (at -0.1 3.86) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_7 smd rect (at -2.9 1.06) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_8 smd rect (at -1.5 1.06) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_9 smd rect (at -0.1 1.06) (size 0.9 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 41_10 thru_hole circle (at -1.5 1.76) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_11 thru_hole circle (at -2.9 1.76) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_12 thru_hole circle (at -0.1 1.76) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_13 thru_hole circle (at -2.9 3.16) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_14 thru_hole circle (at -1.5 3.16) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_15 thru_hole circle (at -0.1 3.16) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_16 thru_hole circle (at -2.2 1.06) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_17 thru_hole circle (at -0.8 1.06) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_18 thru_hole circle (at -2.2 2.46) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_19 thru_hole circle (at -0.8 2.46) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_20 thru_hole circle (at -2.2 3.86) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 41_21 thru_hole circle (at -0.8 3.86) (size 0.4 0.4) (drill 0.2) (layers *.Cu))
  (pad 2 smd rect (at -8.75 -3.99) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at -8.75 -2.72) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at -8.75 -1.45) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at -8.75 -0.18) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at -8.75 1.09) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd rect (at -8.75 2.36) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 8 smd rect (at -8.75 3.63) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 9 smd rect (at -8.75 4.9) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 10 smd rect (at -8.75 6.17) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 11 smd rect (at -8.75 7.44) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 12 smd rect (at -8.75 8.71) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 13 smd rect (at -8.75 9.98) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 14 smd rect (at -8.75 11.25) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 15 smd rect (at -6.985 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 27 smd rect (at 8.75 11.25) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 28 smd rect (at 8.75 9.98) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 29 smd rect (at 8.75 8.71) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 30 smd rect (at 8.75 7.44) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 31 smd rect (at 8.75 6.17) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 32 smd rect (at 8.75 4.9) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 33 smd rect (at 8.75 3.63) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 34 smd rect (at 8.75 2.36) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 35 smd rect (at 8.75 1.09) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 36 smd rect (at 8.75 -0.18) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 37 smd rect (at 8.75 -1.45) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 38 smd rect (at 8.75 -2.72) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 39 smd rect (at 8.75 -3.99) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 40 smd rect (at 8.75 -5.26) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste))
  (pad 16 smd rect (at -5.715 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 17 smd rect (at -4.445 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 18 smd rect (at -3.175 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 19 smd rect (at -1.905 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 20 smd rect (at -0.635 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 21 smd rect (at 0.635 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 22 smd rect (at 1.905 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 23 smd rect (at 3.175 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 24 smd rect (at 4.445 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 25 smd rect (at 5.715 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (pad 26 smd rect (at 6.985 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste))
  (fp_line (start -9.0 -12.75) (end 9.0 -12.75) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 -12.75) (end 9.0 -6.75) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 -6.75) (end 9.0 12.75) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 12.75) (end -9.0 12.75) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 12.75) (end -9.0 -6.75) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 -6.75) (end -9.0 -12.75) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 -6.75) (end 9.0 -6.75) (layer F.Fab) (width 0.127))
  (fp_text user ANTENNA (at -4.5 -9.5) (layer F.Fab)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (fp_line (start -9.75 13.5) (end -9.75 -13.0) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.75 -13.0) (end 9.75 -13.0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.75 -13.0) (end 9.75 13.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.75 13.5) (end 9.75 13.5) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -10.2 -5.26) (end -10.1 -5.26) (layer F.Fab) (width 0.2))
  (fp_line (start -9.0 -12.75) (end 9.0 -12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 -12.75) (end 9.0 -6.03) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 -6.03) (end -9.0 -12.75) (layer F.SilkS) (width 0.127))
  (fp_circle (center -10.2 -5.26) (end -10.1 -5.26) (layer F.SilkS) (width 0.2))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -12.75)
        (xy 9.0 -12.75)
        (xy 9.0 -6.75)
        (xy -9.0 -6.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -12.75)
        (xy 9.0 -12.75)
        (xy 9.0 -6.75)
        (xy -9.0 -6.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -12.75)
        (xy 9.0 -12.75)
        (xy 9.0 -6.75)
        (xy -9.0 -6.75)
      )
    )
  )
  (fp_line (start -9.0 12.02) (end -9.0 12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 12.75) (end -7.755 12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 12.02) (end 9.0 12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 12.75) (end 7.755 12.75) (layer F.SilkS) (width 0.127))
)