(module CalTest_CT3151 (layer F.Cu) (tedit 5BAA5155)
  (descr "Right-angle standard banana jack, http://www.caltestelectronics.com/images/attachments/P315100rH_drawing.pdf")
  (tags "banana jack horizontal")
  (fp_text reference REF** (at 2.54 -5.46) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CalTest_CT3151 (at 2.54 10.54) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5.8 5.8) (end -0.68 5.8) (layer F.Fab) (width 0.1))
  (fp_line (start -0.68 5.8) (end -0.68 7.29) (layer F.Fab) (width 0.1))
  (fp_line (start -0.68 7.29) (end -9.79 9.29) (layer F.Fab) (width 0.1))
  (fp_line (start -9.79 9.29) (end -18.9 9.29) (layer F.Fab) (width 0.1))
  (fp_line (start -18.9 9.29) (end -18.9 8.29) (layer F.Fab) (width 0.1))
  (fp_line (start -18.9 8.29) (end -21.9 8.29) (layer F.Fab) (width 0.1))
  (fp_line (start -21.9 8.29) (end -21.9 -3.21) (layer F.Fab) (width 0.1))
  (fp_line (start -21.9 -3.21) (end -18.9 -3.21) (layer F.Fab) (width 0.1))
  (fp_line (start -18.9 -3.21) (end -18.9 -4.21) (layer F.Fab) (width 0.1))
  (fp_line (start -18.9 -4.21) (end -9.79 -4.21) (layer F.Fab) (width 0.1))
  (fp_line (start -9.79 -4.21) (end -0.68 -2.21) (layer F.Fab) (width 0.1))
  (fp_line (start -0.68 -2.21) (end -0.68 -0.72) (layer F.Fab) (width 0.1))
  (fp_line (start -0.68 -0.72) (end 5.8 -0.72) (layer F.Fab) (width 0.1))
  (fp_line (start 5.8 -0.72) (end 5.8 5.8) (layer F.Fab) (width 0.1))
  (fp_line (start 3.653 5.92) (end 1.417 5.92) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.561 6.703) (end -0.561 7.41) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.561 7.41) (end -9.79 9.41) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.79 9.41) (end -19.02 9.41) (layer F.SilkS) (width 0.12))
  (fp_line (start -19.02 9.41) (end -19.02 8.41) (layer F.SilkS) (width 0.12))
  (fp_line (start -19.02 8.41) (end -22.02 8.41) (layer F.SilkS) (width 0.12))
  (fp_line (start -22.02 8.41) (end -22.02 -3.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -22.02 -3.33) (end -19.02 -3.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -19.02 -3.33) (end -19.02 -4.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -19.02 -4.33) (end -9.79 -4.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.79 -4.33) (end -0.561 -2.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.561 -2.33) (end -0.561 -1.623) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.417 -0.84) (end 3.652 -0.84) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.92 1.425) (end 5.92 3.656) (layer F.SilkS) (width 0.12))
  (fp_line (start -22.4 -4.71) (end -22.4 9.79) (layer F.CrtYd) (width 0.05))
  (fp_line (start -22.4 9.79) (end 6.88 9.79) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.88 9.79) (end 6.88 -4.71) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.88 -4.71) (end -22.4 -4.71) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 5.08) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 5.08 0) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 5.08 5.08) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
  (fp_text user %R (at 2.54 2.54) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Connector.3dshapes/CalTest_CT3151.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)