(module Tag-Connect_TC2050-IDC-NL_2x05_P1.27mm_Vertical (layer F.Cu) (tedit 5E793CF5)
  (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2050-IDC-NL%20Datasheet.pdf")
  (tags "tag connect programming header pogo pins")
  (attr virtual)
  (fp_text reference REF** (at 0 2.9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Tag-Connect_TC2050-IDC-NL_2x05_P1.27mm_Vertical (at 0 4.05) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.175 1.27) (end -3.175 0.635) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.54 1.27) (end -3.175 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.33 0.77) (end -5.33 -0.77) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.63 2.3) (end -3.19 2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.33 -1.6) (end 5.33 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.19 -2.3) (end 4.63 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.54 0.635) (end -2.54 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 2.54 0.635) (end -2.54 0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 2.54 -0.635) (end 2.54 0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -2.54 -0.635) (end 2.54 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -2.54 0.635) (end -1.27 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -2.54 0) (end -1.905 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -1.905 0.635) (end -0.635 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -1.27 0.635) (end 0 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 1.905 0.635) (end 2.54 0) (layer Dwgs.User) (width 0.1))
  (fp_text user KEEPOUT (at 0 0) (layer Cmts.User)
    (effects (font (size 0.4 0.4) (thickness 0.07)))
  )
  (fp_line (start -0.635 0.635) (end 0.635 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 0 0.635) (end 1.27 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 0.635 0.635) (end 1.905 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 1.27 0.635) (end 2.54 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -3.1 -2.05) (end 4.48 -2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.08 -1.45) (end 5.08 1.45) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.48 2.05) (end -3.1 2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.08 0.65) (end -5.08 -0.65) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 2.05) (end -5.08 0.65) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.08 -0.65) (end -3.1 -2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.48 -2.05) (end 5.08 -1.45) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.48 2.05) (end 5.08 1.45) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.45 -3.37) (end 5.453 -3.37) (layer Dwgs.User) (width 0.1))
  (fp_line (start 6.223 -2.6) (end 6.223 2.6) (layer Dwgs.User) (width 0.1))
  (fp_line (start 5.453 3.37) (end -3.45 3.37) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.223 1.4) (end -6.223 -1.4) (layer Dwgs.User) (width 0.1))
  (fp_line (start 5.453 3.37) (end 6.223 2.6) (layer Dwgs.User) (width 0.1))
  (fp_line (start 5.453 -3.37) (end 6.223 -2.6) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.223 -1.4) (end -3.45 -3.37) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.223 1.4) (end -3.45 3.37) (layer Dwgs.User) (width 0.1))
  (fp_line (start -3.1 -2.05) (end 4.48 -2.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start 5.08 -1.45) (end 5.08 1.45) (layer Dwgs.User) (width 0.1))
  (fp_line (start 4.48 2.05) (end -3.1 2.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.08 0.65) (end -5.08 -0.65) (layer Dwgs.User) (width 0.1))
  (fp_line (start -3.1 2.05) (end -5.08 0.65) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.08 -0.65) (end -3.1 -2.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start 4.48 -2.05) (end 5.08 -1.45) (layer Dwgs.User) (width 0.1))
  (fp_line (start 4.48 2.05) (end 5.08 1.45) (layer Dwgs.User) (width 0.1))
  (fp_text user "6.35mm Z-KEEPOUT" (at 1 -2.75) (layer Cmts.User)
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_text user "6.35mm Z-KEEPOUT" (at 1 2.75) (layer Cmts.User)
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_line (start -6.223 -1.4) (end -5.1 -0.277) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.4 -1.9) (end -4.55 -1.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start -4.6 -2.5) (end -3.75 -1.65) (layer Dwgs.User) (width 0.1))
  (fp_line (start -3.75 -3.15) (end -2.65 -2.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start -2.15 -3.35) (end -0.85 -2.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start -0.5 -3.35) (end 0.8 -2.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start 1.4 -3.35) (end 2.7 -2.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start 3.15 -3.35) (end 4.4 -2.1) (layer Dwgs.User) (width 0.1))
  (fp_line (start 4.4 -2.1) (end 4.45 -2.05) (layer Dwgs.User) (width 0.1))
  (fp_line (start 4.55 -3.35) (end 6.2 -1.7) (layer Dwgs.User) (width 0.1))
  (fp_line (start 5.08 -1.45) (end 6.2 -0.33) (layer Dwgs.User) (width 0.1))
  (fp_line (start 5.1 0.05) (end 6.2 1.15) (layer Dwgs.User) (width 0.1))
  (fp_line (start 5.1 1.45) (end 6.2 2.55) (layer Dwgs.User) (width 0.1))
  (fp_line (start 4.2 2.1) (end 5.45 3.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start 2.7 2.05) (end 4 3.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start 1.15 2.05) (end 2.45 3.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start -0.35 2.1) (end 0.9 3.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start -2.1 2.05) (end -0.8 3.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.2 -0.25) (end -2.6 3.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start -6.2 0.6) (end -3.45 3.35) (layer Dwgs.User) (width 0.1))
  (fp_line (start -3.19 2.3) (end -5.33 0.77) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.33 -0.77) (end -3.19 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.63 -2.3) (end 5.33 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.63 2.3) (end 5.33 1.6) (layer F.CrtYd) (width 0.05))
  (pad "" np_thru_hole circle (at 3.81 -1.016) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 3.81 1.016) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -3.81 0) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 1 connect circle (at -2.54 0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 2 connect circle (at -1.27 0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 3 connect circle (at 0 0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 4 connect circle (at 1.27 0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 5 connect circle (at 2.54 0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 6 connect circle (at 2.54 -0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 7 connect circle (at 1.27 -0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 8 connect circle (at 0 -0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 9 connect circle (at -1.27 -0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 10 connect circle (at -2.54 -0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
)
