(module GB042-34S-H10 (layer F.Cu) (tedit 5B5CA0A1)
  (descr http://www.lsmtron.com/pdf/Connector&Antenna_catalog.PDF)
  (tags "34pin SMD connector ")
  (attr smd)
  (fp_text reference REF** (at 0 -5.55) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value GB042-34S-H10 (at 0 0 270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.9 -4.8) (end 2.1 -4.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.1 -4.8) (end 2.1 -3.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.1 4.8) (end -2.1 4.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.1 4.8) (end 2.1 3.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.95 -4.65) (end 1.95 4.65) (layer F.Fab) (width 0.1))
  (fp_line (start 1.95 4.65) (end -1.95 4.65) (layer F.Fab) (width 0.1))
  (fp_line (start -1.95 4.65) (end -1.95 -3.65) (layer F.Fab) (width 0.1))
  (fp_line (start -0.95 -4.65) (end 1.95 -4.65) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 -5.55) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.45 -4.9) (end 2.45 4.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.45 4.9) (end -2.45 4.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.45 4.9) (end -2.45 -4.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.45 -4.9) (end 2.45 -4.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.95 -3.65) (end -0.95 -4.65) (layer F.Fab) (width 0.1))
  (fp_line (start -2.1 4.8) (end -2.1 3.8) (layer F.SilkS) (width 0.15))
  (pad 34 smd rect (at 1.7 -3.2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.7 -3.2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 1.7 -2.8 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.7 -2.8 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 1.7 -2.4 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.7 -2.4 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 1.7 -2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.7 -2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 1.7 -1.6 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.7 -1.6 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 1.7 -1.2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.7 -1.2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 1.7 -0.8 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -1.7 -0.8 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 1.7 -0.4 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.7 -0.4 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 1.7 0 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.7 0 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 1.7 0.4 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -1.7 0.4 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 1.7 0.8 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.7 0.8 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 1.7 1.2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -1.7 1.2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 1.7 1.6 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -1.7 1.6 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 1.7 2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -1.7 2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 1.7 2.4 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -1.7 2.4 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 1.7 2.8 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -1.7 2.8 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 1.7 3.2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -1.7 3.2 270) (size 0.23 1) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector.3dshapes/GB042-34S-H10.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
