(module Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical (layer F.Cu) (tedit 5A29CEA9)
  (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
  (tags "tag connect programming header pogo pins")
  (attr virtual)
  (fp_text reference REF** (at 0 2.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical (at 0 -2.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.905 1.27) (end -1.905 0.635) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 1.27) (end -1.905 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.5 2) (end -3.5 -2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.5 2) (end -3.5 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.5 -2) (end 3.5 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.5 -2) (end 3.5 -2) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.27 0.635) (end -1.27 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 1.27 0.635) (end -1.27 0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 1.27 -0.635) (end 1.27 0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -1.27 -0.635) (end 1.27 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -1.27 0.635) (end 0 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -1.27 0) (end -0.635 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start -0.635 0.635) (end 0.635 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 0 0.635) (end 1.27 -0.635) (layer Dwgs.User) (width 0.1))
  (fp_line (start 0.635 0.635) (end 1.27 0) (layer Dwgs.User) (width 0.1))
  (fp_text user KEEPOUT (at 0 0) (layer Cmts.User)
    (effects (font (size 0.4 0.4) (thickness 0.07)))
  )
  (pad "" np_thru_hole circle (at 2.54 -1.016) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 2.54 1.016) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -2.54 0) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 1 connect circle (at -1.27 0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 2 connect circle (at -1.27 -0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 3 connect circle (at 0 0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 4 connect circle (at 0 -0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 5 connect circle (at 1.27 0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
  (pad 6 connect circle (at 1.27 -0.635) (size 0.7874 0.7874) (layers F.Cu F.Mask))
)
