<?xml version="1.0" encoding="UTF-8"?>
<Repetier-Firmware-EEPROM>
	<epr pos="75" type="2" value="250000">Baudrate</epr>
	<epr pos="43" type="1" value="1">Advanced User</epr>
	<epr pos="129" type="3" value="1960.118">Filament printed [m]</epr>
	<epr pos="125" type="2" value="487643">Printer active [s]</epr>
	<epr pos="79" type="2" value="900000">Max. inactive time [ms,0=off]</epr>
	<epr pos="83" type="2" value="600000">Stop stepper after inactivity [ms,0=off]</epr>
	<epr pos="11" type="3" value="80.0000">Steps per mm</epr>
	<epr pos="23" type="3" value="250.000">Max. feedrate [mm/s]</epr>
	<epr pos="35" type="3" value="80.000">Homing feedrate [mm/s]</epr>
	<epr pos="39" type="3" value="32.000">Max. jerk [mm/s]</epr>
	<epr pos="133" type="3" value="0.000">X home pos [mm]</epr>
	<epr pos="137" type="3" value="0.000">Y home pos [mm]</epr>
	<epr pos="141" type="3" value="0.000">Z home pos [mm]</epr>
	<epr pos="145" type="3" value="250.000">X max length [mm]</epr>
	<epr pos="149" type="3" value="250.000">Y max length [mm]</epr>
	<epr pos="153" type="3" value="396.737">Z max length [mm]</epr>
	<epr pos="59" type="3" value="1850.000">Acceleration [mm/s^2]</epr>
	<epr pos="71" type="3" value="3000.000">Travel acceleration [mm/s^2]</epr>
	<epr pos="881" type="3" value="291.060">Diagonal rod length [mm]</epr>
	<epr pos="885" type="3" value="143.799">Horizontal rod radius at 0,0 [mm]</epr>
	<epr pos="925" type="3" value="145.000">Max printable radius [mm]</epr>
	<epr pos="891" type="1" value="80">Segments/s for travel</epr>
	<epr pos="889" type="1" value="200">Segments/s for printing</epr>
	<epr pos="893" type="1" value="24">Tower X endstop offset [steps]</epr>
	<epr pos="895" type="1" value="0">Tower Y endstop offset [steps]</epr>
	<epr pos="897" type="1" value="58">Tower Z endstop offset [steps]</epr>
	<epr pos="901" type="3" value="210.000">Alpha A(210):</epr>
	<epr pos="905" type="3" value="330.000">Alpha B(330):</epr>
	<epr pos="909" type="3" value="90.000">Alpha C(90):</epr>
	<epr pos="913" type="3" value="0.000">Delta Radius A(0):</epr>
	<epr pos="917" type="3" value="0.000">Delta Radius B(0):</epr>
	<epr pos="921" type="3" value="0.000">Delta Radius C(0):</epr>
	<epr pos="933" type="3" value="0.000">Corr. diagonal A [mm]</epr>
	<epr pos="937" type="3" value="0.000">Corr. diagonal B [mm]</epr>
	<epr pos="941" type="3" value="0.000">Corr. diagonal C [mm]</epr>
	<epr pos="808" type="3" value="-0.100">Z-probe height [mm]</epr>
	<epr pos="929" type="3" value="20.000">Max. z-probe - bed dist. [mm]</epr>
	<epr pos="812" type="3" value="80.000">Z-probe speed [mm/s]</epr>
	<epr pos="840" type="3" value="50.000">Z-probe x-y-speed [mm/s]</epr>
	<epr pos="800" type="3" value="0.000">Z-probe offset x [mm]</epr>
	<epr pos="804" type="3" value="0.000">Z-probe offset y [mm]</epr>
	<epr pos="816" type="3" value="-123.565">Z-probe X1</epr>
	<epr pos="820" type="3" value="-71.340">Z-probe Y1</epr>
	<epr pos="824" type="3" value="123.565">Z-probe X2</epr>
	<epr pos="828" type="3" value="-71.340">Z-probe Y2</epr>
	<epr pos="832" type="3" value="0.000">Z-probe X3</epr>
	<epr pos="836" type="3" value="142.680">Z-probe Y3</epr>
	<epr pos="880" type="0" value="1">Autolevel active (1/0)</epr>
	<epr pos="106" type="0" value="1">Bed Heat Manager [0-3]</epr>
	<epr pos="107" type="0" value="255">Bed PID drive max</epr>
	<epr pos="124" type="0" value="80">Bed PID drive min</epr>
	<epr pos="108" type="3" value="87.860">Bed PID P-gain</epr>
	<epr pos="112" type="3" value="3.010">Bed PID I-gain</epr>
	<epr pos="116" type="3" value="641.820">Bed PID D-gain</epr>
	<epr pos="120" type="0" value="255">Bed PID max value [0-255]</epr>
	<epr pos="200" type="3" value="92.400">Extr.1 steps per mm</epr>
	<epr pos="204" type="3" value="100.000">Extr.1 max. feedrate [mm/s]</epr>
	<epr pos="208" type="3" value="45.000">Extr.1 start feedrate [mm/s]</epr>
	<epr pos="212" type="3" value="6500.000">Extr.1 acceleration [mm/s^2]</epr>
	<epr pos="216" type="0" value="1">Extr.1 heat manager [0-3]</epr>
	<epr pos="217" type="0" value="230">Extr.1 PID drive max</epr>
	<epr pos="245" type="0" value="80">Extr.1 PID drive min</epr>
	<epr pos="218" type="3" value="48.3000">Extr.1 PID P-gain/dead-time</epr>
	<epr pos="222" type="3" value="9.7000">Extr.1 PID I-gain</epr>
	<epr pos="226" type="3" value="60.0000">Extr.1 PID D-gain</epr>
	<epr pos="230" type="0" value="255">Extr.1 PID max value [0-255]</epr>
</Repetier-Firmware-EEPROM>
