var debugMode = false;              // debug mode
var sendPrintCommands = true;       // if Doodle3d should send print commands to the 3d printer
var communicateWithWifibox = true;  // if Doodle3d should try interfacing with the wifibox (in case one is not connected)
var wifiboxIsRemote = false;        // when you want to run the client on a computer and have it remotely connect to the wifibox
var autoUpdate = true; 							// auto retrieve updates about temperature and progress from printer

var printer =  new Printer();
var progressbar = new Progressbar();
var thermometer = new Thermometer();
var settingsWindow = new SettingsWindow();
var message = new Message();

var firstTimeSettingsLoaded = true;

var wifiboxURL; // Using the uhttpd lua handler as default, because of better performance
var wifiboxCGIBinURL; // CGI-bin, for some network stuff, where it needs to restart the webserver for example

var $drawAreaContainer, $doodleCanvas, doodleCanvas, doodleCanvasContext, $previewContainer;

$(function() {
  console.log("ready");


  //TODO give this a more logical place in code

  if (getURLParameter("d") != "null") debugMode = (getURLParameter("d") == "1");
  if (getURLParameter("p") != "null") sendPrintCommands = (getURLParameter("p") == "1");
  if (getURLParameter("c") != "null") communicateWithWifibox = (getURLParameter("c") == "1");
  if (getURLParameter("r") != "null") wifiboxIsRemote = (getURLParameter("r") == "1");
  if (getURLParameter("u") != "null") autoUpdate = (getURLParameter("u") == "1");
  
	if (wifiboxIsRemote) {
		wifiboxURL = "http://192.168.5.1/d3dapi";
		wifiboxCGIBinURL = "http://192.168.5.1/cgi-bin/d3dapi";
	} else {
		wifiboxURL = "http://" + window.location.host + "/d3dapi";
		wifiboxCGIBinURL = "http://" + window.location.host + "/cgi-bin/d3dapi";
	}

  if (!communicateWithWifibox) {
    sendPrintCommands = false; // 'communicateWithWifibox = false' implies this
  }
  console.log("debugMode: " + debugMode);
  console.log("sendPrintCommands: " + sendPrintCommands);
  console.log("communicateWithWifibox: " + communicateWithWifibox);
  console.log("wifiboxIsRemote: " + wifiboxIsRemote);
  console.log("wifibox URL: " + wifiboxURL);

  initDoodleDrawing();
  initPreviewRendering();
  initLayouting();
  initSidebars();
  initButtonBehavior();
  initVerticalShapes();

	thermometer.init($("#thermometerCanvas"), $("#thermometerContainer"));
  progressbar.init($("#progressbarCanvas"), $("#progressbarCanvasContainer"));

  message.init($("#message"));
  
  printer.init();
	$(document).on(Printer.UPDATE,update);

	settingsWindow.init(wifiboxURL,wifiboxCGIBinURL);
	$(document).on(SettingsWindow.SETTINGS_LOADED, settingsLoaded);

  if(debugMode) {
    console.log("debug mode is true");
    $("body").css("overflow", "auto");
    $("#debug_textArea").css("display", "block");
    $("#preview_tmp").css("display", "block");
    
    $("#debug_display").css("display", "block");

    // show and hide the progressguage and thermometer
    showhideInterval = setInterval(showOrHideThermo, 2500);

//    $("#debugContainer").css("display", "block");

    /* TEMP CODE!! -> artificially populates the startgcode and endgcode textareas in the settings window */
    // todo remove this temporary code...
    /*
    setTimeout(function() {
      $("#startgcode").text("");
      $("#startgcode").append("G21 (mm) \n");
      $("#startgcode").append("G91 (relative) \n");
      $("#startgcode").append("G28 X0 Y0 Z0 (physical home) \n");
      $("#startgcode").append("M104 S230 (temperature) \n");
      $("#startgcode").append("G1 E10 F250 (flow) \n");
      $("#startgcode").append("G92 X-100 Y-100 Z0 E10 \n");
      $("#startgcode").append("G1 Z3 F5000 (prevent diagonal line) \n");
      $("#startgcode").append("G90 (absolute) \n");
      $("#startgcode").append("M106 (fan on)");
      console.log("$('#startgcode'): " + $("#startgcode").val());

      $("#endgcode").text("");
      $("#endgcode").append("G1 X-100 Y-100 F15000 (fast homing) \n");
      $("#endgcode").append("M107 \n");
      $("#endgcode").append("M84 (disable axes) \n");
      console.log("$('#endgcode'): " + $("#endgcode").val());
    }, 1000);
    //*/
  }
<<<<<<< .merge_file_HNcA77
=======
  //showhideInterval = setInterval(showOrHideThermo, 2500);
>>>>>>> .merge_file_0hlg7g
});

/*var showhideInterval;
var showOrHide = false;

function showOrHideThermo() {
  console.log("f:showOrHideThermo()");
  if (showOrHide) {
    thermometer.hide();
    progressbar.hide();
  } else {
    thermometer.show();
    progressbar.show();

  }
  showOrHide = !showOrHide;
}*/

function settingsLoaded() {
	console.log("settingsLoaded");
	console.log("autoHeatup: ",settings["printer.heatup.enabled"]);
	if(settings["printer.heatup.enabled"]) {
		if(firstTimeSettingsLoaded) {
			printer.preheat();
			firstTimeSettingsLoaded = false;
		}
	}
}

function setDebugText(text) {
	$("#debug_display").text(text);
}
