(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "S2B-PH-SM4-TB(LF)(SN)" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -5.08 5.588 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "S2B-PH-SM4-TB(LF)(SN)" (id 1) (at -5.08 -9.4234 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "JST_S2B-PH-SM4-TB(LF)(SN)" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendation" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "JST" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "S2B-PH-SM4-TB(LF)(SN)_0_0"
      (rectangle (start -5.08 -7.62) (end 5.08 5.08)
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin passive line (at -7.62 2.54 0) (length 2.54)
        (name "1" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -7.62 0 0) (length 2.54)
        (name "2" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -7.62 -5.08 0) (length 2.54)
        (name "SHIELD" (effects (font (size 1.016 1.016))))
        (number "S1" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -7.62 -5.08 0) (length 2.54)
        (name "SHIELD" (effects (font (size 1.016 1.016))))
        (number "S2" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
