(footprint "Antenna_Cap" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 77006be8-e871-4875-98bd-df9b9f9c71da)
  )
  (fp_text value "Antenna_Cap" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d012688b-7a14-45be-8853-ccc0dc10dc71)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 880d94e0-447e-413a-a558-cee4b897ff70)
  )
  (pad "1" smd oval (at 18.034 5.461) (size 20.32 5.334) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 92f3f87e-5e1a-419d-afde-68dd17a44605))
  (pad "2" smd oval (at 18.288 29.972) (size 20.32 5.334) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9cb2aa88-c3a2-4cc1-bdd9-a23918a92f25))
)
