(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "TPS63060DSCT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 18.542 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "TPS63060DSCT" (id 1) (at -12.7 -18.542 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "CONV_TPS63060DSCT" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PARTREV" "B" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "Texas Instruments" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "0.8 mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "TPS63060DSCT_0_0"
      (rectangle (start -12.7 -17.78) (end 12.7 17.78)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin passive line (at -17.78 -5.08 0) (length 5.08)
        (name "L1" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -17.78 -7.62 0) (length 5.08)
        (name "L2" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "PGND" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 15.24 0) (length 5.08)
        (name "VIN" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 10.16 0) (length 5.08)
        (name "EN" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 5.08 0) (length 5.08)
        (name "PS/SYNC" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 17.78 5.08 180) (length 5.08)
        (name "PG" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -17.78 0 0) (length 5.08)
        (name "VAUX" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -12.7 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 17.78 10.16 180) (length 5.08)
        (name "FB" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 17.78 15.24 180) (length 5.08)
        (name "VOUT" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
