(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ESP32-C3-WROOM-02-H4" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 21.082 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "ESP32-C3-WROOM-02-H4" (id 1) (at -12.7 -18.542 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "MODULE_ESP32-C3-WROOM-02-H4" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.35 mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "Espressif" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PARTREV" "V1.0" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "ESP32-C3-WROOM-02-H4_0_0"
      (rectangle (start -12.7 -17.78) (end 12.7 20.32)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 17.78 17.78 180) (length 5.08)
        (name "3V3" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 2.54 180) (length 5.08)
        (name "IO10" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -12.7 0) (length 5.08)
        (name "RXD" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -10.16 0) (length 5.08)
        (name "TXD" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 0 180) (length 5.08)
        (name "IO18" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -2.54 180) (length 5.08)
        (name "IO19" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 2.54 0) (length 5.08)
        (name "IO3" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 5.08 0) (length 5.08)
        (name "IO2" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 7.62 0) (length 5.08)
        (name "IO1" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 10.16 0) (length 5.08)
        (name "IO0" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 15.24 0) (length 5.08)
        (name "EN" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 0 0) (length 5.08)
        (name "IO4" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "34" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "37" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "38" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "39" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -2.54 0) (length 5.08)
        (name "IO5" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -5.08 0) (length 5.08)
        (name "IO6" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 10.16 180) (length 5.08)
        (name "IO7" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 7.62 180) (length 5.08)
        (name "IO8" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 5.08 180) (length 5.08)
        (name "IO9" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
