(module NS-Tech_Grove_1x04_P2mm_Vertical (layer F.Cu) (tedit 5A2A5779)
  (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
  (tags Grove-1x04)
  (fp_text reference REF** (at -1.5 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value NS-Tech_Grove_1x04_P2mm_Vertical (at 4.19 2.83 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at -2 2 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.9 0) (end 2.2 1) (layer F.Fab) (width 0.1))
  (fp_line (start 2.2 -1) (end 0.9 0) (layer F.Fab) (width 0.1))
  (fp_line (start 3 -3) (end 3 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -3) (end 3 -3) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.45 -2.65) (end -3.45 8.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.45 8.7) (end 2.7 8.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.7 8.7) (end 2.7 -2.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.45 -2.65) (end 2.7 -2.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.3 5) (end -3.3 5.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 0.4) (end -3.3 1) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.55 -2.5) (end 2.55 8.55) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 -2.5) (end 2.55 -2.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 1.25) (end -3.3 4.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 8.55) (end 2.55 8.55) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 -2.5) (end -3.3 0.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 5.9) (end -3.3 8.55) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.9 -2.1) (end 2.2 -2.1) (layer F.Fab) (width 0.1))
  (fp_line (start 2.2 -2.1) (end 2.2 8.1) (layer F.Fab) (width 0.1))
  (fp_line (start 2.2 8.1) (end -2.9 8.1) (layer F.Fab) (width 0.1))
  (fp_line (start -2.9 8.1) (end -2.9 -2.1) (layer F.Fab) (width 0.1))
  (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 4) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector.3dshapes/NS-Tech_Grove_1x04_P2mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.3937 0.3937 0.3937))
    (rotate (xyz 0 0 -90))
  )
)
