(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ESP32-S3-WROOM-1-N16R2" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 34.1122 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "ESP32-S3-WROOM-1-N16R2" (id 1) (at -10.16 -35.56 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "XCVR_ESP32-S3-WROOM-1-N16R2" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.25mm" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PARTREV" "v1.0" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "Espressif" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "ESP32-S3-WROOM-1-N16R2_0_0"
      (rectangle (start -10.16 -33.02) (end 10.16 33.02)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 5.08)
        (name "IO17" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 5.08)
        (name "IO18" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 5.08)
        (name "IO8" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 5.08)
        (name "IO19" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 5.08)
        (name "IO20" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 7.62 0) (length 5.08)
        (name "IO3" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -20.32 180) (length 5.08)
        (name "IO46" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 5.08)
        (name "IO9" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 5.08)
        (name "IO10" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 5.08)
        (name "IO11" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 30.48 180) (length 5.08)
        (name "3V3" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -15.24 0) (length 5.08)
        (name "IO12" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -17.78 0) (length 5.08)
        (name "IO13" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -20.32 0) (length 5.08)
        (name "IO14" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 5.08)
        (name "IO21" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -22.86 180) (length 5.08)
        (name "IO47" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -25.4 180) (length 5.08)
        (name "IO48" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -17.78 180) (length 5.08)
        (name "IO45" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 15.24 0) (length 5.08)
        (name "IO0" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 5.08)
        (name "IO35" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 5.08)
        (name "IO36" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 27.94 0) (length 5.08)
        (name "EN" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 5.08)
        (name "IO37" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 5.08)
        (name "IO38" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 5.08)
        (name "IO39" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 5.08)
        (name "IO40" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -12.7 180) (length 5.08)
        (name "IO41" (effects (font (size 1.016 1.016))))
        (number "34" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 15.24 -15.24 180) (length 5.08)
        (name "IO42" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 22.86 0) (length 5.08)
        (name "RXD0" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 20.32 0) (length 5.08)
        (name "TXD0" (effects (font (size 1.016 1.016))))
        (number "37" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 10.16 0) (length 5.08)
        (name "IO2" (effects (font (size 1.016 1.016))))
        (number "38" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 5.08)
        (name "IO1" (effects (font (size 1.016 1.016))))
        (number "39" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 5.08 0) (length 5.08)
        (name "IO4" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "40" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_1" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_2" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_3" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_4" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_5" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_6" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_7" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_8" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -30.48 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "41_9" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 2.54 0) (length 5.08)
        (name "IO5" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 5.08)
        (name "IO6" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 5.08)
        (name "IO7" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -22.86 0) (length 5.08)
        (name "IO15" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -15.24 -25.4 0) (length 5.08)
        (name "IO16" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
