<?xml version="1.0" encoding="UTF-8"?>
<inkscape-extension xmlns="http://www.inkscape.org/namespace/inkscape/extension">
    <name>TXT file output</name>
    <id>org.inkstitch.output.txt.de_DE</id>
    <dependency type="executable" location="extensions">inkstitch.py</dependency>
    <dependency type="executable" location="extensions">inkex.py</dependency>
    <output>
        <extension>.txt</extension>
        <mimetype>application/x-embroidery-txt</mimetype>
        <_filetypename>Ink/Stitch: G-Code Format (.txt)</_filetypename>
        <_filetypetooltip>Speichern des Designs ins TXT Format mit Ink/Stitch</_filetypetooltip>
        <dataloss>true</dataloss>
    </output>
    <param name="extension" type="string" gui-hidden="true">output</param>
    <param name="format" type="string" gui-hidden="true">txt</param>
    
        
    <param name="laser_mode" type="boolean" gui-text="Lasermodus" gui-description="Laser mode (generate g-code for grbl laser mode)">false</param>
    <param name="dynamic_laser_power" type="boolean" gui-text="dynamic laser power" gui-description="Use Grbl&#39;s M4 dynamic laser power mode.  Ensures consistent laser cutting power regardless of motor speed.  Only for PWM-capable lasers." min="0.0" max="5.0">true</param>
    <param name="laser_warm_up_time" type="float" gui-text="Laser Aufwärmzeit" gui-description="Warte so viele Sekunden nach dem Einschalten des Lasers - Aufwärmphase (G4 Befehl)">0.0</param>
    <param name="flip_x" type="boolean" gui-text="negate X coordinate values" gui-description="X-Koordinaten negieren">false</param>
    <param name="flip_y" type="boolean" gui-text="negate Y coordinate values" gui-description="Y-Koordinaten negieren">false</param>
    <param name="stitch_z_travel" type="float" gui-text="Z travel per stitch" gui-description="Erhöhe z-Koordinate um diesen Wert pro Stich">5.0</param>
    <param name="spindle_speed" type="int" gui-text="spindle speed" gui-description="spindle speed (laser power for laser mode, set to -1 to omit)" min="-1" max="1000000000">-1</param>
    <param name="min_spindle_speed" type="int" gui-text="min spindle speed" gui-description="minimum spindle speed value (grbl $31 setting)" min="-1" max="1000000000">-1</param>
    <param name="max_spindle_speed" type="int" gui-text="max spindle speed" gui-description="minimum spindle speed value (grbl $30 setting)" min="-1" max="1000000000">-1</param>
    <param name="feed_rate" type="int" gui-description="feed rate (in mm/min, set to -1 to omit)" min="-1" max="1000000000">-1</param>
    <script>
        <command reldir="extensions" interpreter="python">inkstitch.py</command>
    </script>
</inkscape-extension>
